{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["1.DOC Factor ","2. Area oputput factor","3. QA field test"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"1.DOC Factor ","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[[6,0,6,5],[10,0,10,5]]}
["測定日："]
["測定者："]
[]
[]
[]
[]
["A) 基準深（線量最⼤深）の100MUあたりの線量"]
[null,"4MV","6MV","10MV","6FFF","10FFF"]
["Gy / 100MU"]
[]
["B) 基準条件におけるIQMのシグナル値"]
[null,"4MV","6MV","10MV","6FFF","10FFF"]
["Quick beam, 20x20, 200MU (1回目)"]
["Quick beam, 20x20, 200MU (2回目)"]
["Quick beam, 20x20, 200MU (3回目)"]

{"sheet":"2. Area oputput factor","index":1,"n_rows":64,"n_cols":13,"rows_kept":64,"cut":false,"hidden":false,"merged":[[5,0,5,5],[5,7,5,12]]}
["測定日：","2024-05-16",null,null,null,null,null,"測定日："]
["測定者：",null,null,null,null,null,null,"測定者："]
["Mosaiqに登録されたPatient ID : ",null,null,null,null,null,null,"Mosaiqに登録されたPatient ID : "]
[]
[]
["Dynamic AOF チェックシート",null,null,null,null,null,null,"Static AOF チェックシート"]
[null,"4MV","6MV","10MV","6FFF","10FFF",null,null,"4MV","6MV","10MV","6FFF","10FFF"]
["Quick beam, 20x20, 200MU(Start)",null,null,null,null,null,null,"Quick beam, 20x20, 200MU (Start)"]
["Field ID: AOF1",null,null,null,null,null,null,"Field ID: Y=05, 500MU"]
["Field ID: AOF2",null,null,null,null,null,null,"Field ID: Y=075, 350MU"]
["Field ID: AOF3",null,null,null,null,null,null,"Field ID: Y=1, 550MU"]
["Field ID: AOF4",null,null,null,null,null,null,"Field ID: Y=2, 450MU"]
["Field ID: AOF5",null,null,null,null,null,null,"Field ID: Y=3, 650MU"]
["Field ID: AOF6",null,null,null,null,null,null,"Field ID: Y=4, 650MU"]
["Field ID: AOF7",null,null,null,null,null,null,"Field ID: Y=5, 750MU"]
["Field ID: AOF8",null,null,null,null,null,null,"Field ID: Y=6, 850MU"]
["Field ID: AOF9",null,null,null,null,null,null,"Field ID: Y=8, 900MU"]
["Field ID: AOF10",null,null,null,null,null,null,"Field ID: Y=10, 900MU"]
["Field ID: AOF11",null,null,null,null,null,null,"Field ID: Y=12, 900MU"]
["Field ID: AOF12",null,null,null,null,null,null,"Field ID: Y=15, 900MU"]
["Field ID: AOF13",null,null,null,null,null,null,"Field ID: Y=20, 900MU"]
["Field ID: AOF14",null,null,null,null,null,null,"Field ID: Y=25, 650MU"]
["Field ID: AOF15",null,null,null,null,null,null,"Field ID: Y=30, 700MU"]
["Quick beam, 20x20, 200MU (End)",null,null,null,null,null,null,"Field ID: Y=35, 550MU"]
["Quick beam, 20x20, 200MU(Start)",null,null,null,null,null,null,"Field ID: Y=40, 650MU"]
["Field ID: AOF1",null,null,null,null,null,null,"Quick beam, 20x20, 200MU (End)"]
["Field ID: AOF2",null,null,null,null,null,null,"Quick beam, 20x20, 200MU (Start)"]
["Field ID: AOF3",null,null,null,null,null,null,"Field ID: Y=05, 500MU"]
["Field ID: AOF4",null,null,null,null,null,null,"Field ID: Y=075, 350MU"]
["Field ID: AOF5",null,null,null,null,null,null,"Field ID: Y=1, 550MU"]
["Field ID: AOF6",null,null,null,null,null,null,"Field ID: Y=2, 450MU"]
["Field ID: AOF7",null,null,null,null,null,null,"Field ID: Y=3, 650MU"]
["Field ID: AOF8",null,null,null,null,null,null,"Field ID: Y=4, 650MU"]
["Field ID: AOF9",null,null,null,null,null,null,"Field ID: Y=5, 750MU"]
["Field ID: AOF10",null,null,null,null,null,null,"Field ID: Y=6, 850MU"]
["Field ID: AOF11",null,null,null,null,null,null,"Field ID: Y=8, 900MU"]
["Field ID: AOF12",null,null,null,null,null,null,"Field ID: Y=10, 900MU"]
["Field ID: AOF13",null,null,null,null,null,null,"Field ID: Y=12, 900MU"]
["Field ID: AOF14",null,null,null,null,null,null,"Field ID: Y=15, 900MU"]
["Field ID: AOF15",null,null,null,null,null,null,"Field ID: Y=20, 900MU"]
["Quick beam, 20x20, 200MU (End)",null,null,null,null,null,null,"Field ID: Y=25, 650MU"]
["Quick beam, 20x20, 200MU(Start)",null,null,null,null,null,null,"Field ID: Y=30, 700MU"]
["Field ID: AOF1",null,null,null,null,null,null,"Field ID: Y=35, 550MU"]
["Field ID: AOF2",null,null,null,null,null,null,"Field ID: Y=40, 650MU"]
["Field ID: AOF3",null,null,null,null,null,null,"Quick beam, 20x20, 200MU (End)"]
["Field ID: AOF4",null,null,null,null,null,null,"Quick beam, 20x20, 200MU (Start)"]
["Field ID: AOF5",null,null,null,null,null,null,"Field ID: Y=05, 500MU"]
["Field ID: AOF6",null,null,null,null,null,null,"Field ID: Y=075, 350MU"]
["Field ID: AOF7",null,null,null,null,null,null,"Field ID: Y=1, 550MU"]
["Field ID: AOF8",null,null,null,null,null,null,"Field ID: Y=2, 450MU"]
["Field ID: AOF9",null,null,null,null,null,null,"Field ID: Y=3, 650MU"]
["Field ID: AOF10",null,null,null,null,null,null,"Field ID: Y=4, 650MU"]
["Field ID: AOF11",null,null,null,null,null,null,"Field ID: Y=5, 750MU"]
["Field ID: AOF12",null,null,null,null,null,null,"Field ID: Y=6, 850MU"]
["Field ID: AOF13",null,null,null,null,null,null,"Field ID: Y=8, 900MU"]
["Field ID: AOF14",null,null,null,null,null,null,"Field ID: Y=10, 900MU"]
["Field ID: AOF15",null,null,null,null,null,null,"Field ID: Y=12, 900MU"]
["Quick beam, 20x20, 200MU (End)",null,null,null,null,null,null,"Field ID: Y=15, 900MU"]
[null,null,null,null,null,null,null,"Field ID: Y=20, 900MU"]
[null,null,null,null,null,null,null,"Field ID: Y=25, 650MU"]
[null,null,null,null,null,null,null,"Field ID: Y=30, 700MU"]
[null,null,null,null,null,null,null,"Field ID: Y=35, 550MU"]
[null,null,null,null,null,null,null,"Field ID: Y=40, 650MU"]
[null,null,null,null,null,null,null,"Quick beam, 20x20, 200MU (End)"]

{"sheet":"3. QA field test","index":2,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":false,"merged":[[5,0,5,5]]}
["測定日："]
["測定者："]
["Mosaiqに登録されたPatient ID : "]
[]
[]
["QA field test チェックシート"]
[null,"4MV","6MV","10MV","6FFF","10FFF"]
["Quick beam, 20x20, 200MU(Start)"]
["Field ID: AGQA4, 3100MU"]
["Quick beam, 20x20, 200MU (End)"]
["Quick beam, 20x20, 200MU(Start)"]
["Field ID: AGQA4, 3100MU"]
["Quick beam, 20x20, 200MU (End)"]